|  |
| --- |
| **5-302.12 Inspection and Cleaning Port, Protected and Secured.**  If a water tank is designed with an access port for inspection and cleaning, the opening shall be in the top of the tank and: |
|  |
| (A) Flanged upward at least 13 mm (one-half inch); and |
|  |
| (B) Equipped with a port cover assembly that is: |
|  |
| (1) Provided with a gasket and a device for securing the cover in place, and |
|  |
| (2) Flanged to overlap the opening and sloped to drain. |