|  |
| --- |
| **4-202.17 Kick Plates, Removable.**  Kick plates shall be designed so that the areas behind them are accessible for inspection and cleaning by being: |
|  |
| (A) Removable by one of the methods specified under Subparagraph 4‑202.11(A)(5) or capable of being rotated open; and |
|  |
| (B) Removable or capable of being rotated open without unlocking equipment doors. |