|  |  |  |
| --- | --- | --- |
| ***Lighting*** |  | **6-303.11 Intensity.**  The light intensity shall be: |
|  |  |  |
|  |  | (A) At least 108 lux (10 foot candles) at a distance of 75 cm (30 inches) above the floor, in walk-in refrigeration units and dry food storage areas and in other areas and rooms during periods of cleaning; |
|  |  |  |
|  |  | (B) At least 215 lux (20 foot candles): |
|  |  |  |
|  |  | (1) At a surface where food is provided for consumer self-service such as buffets and salad bars or where fresh produce or packaged foods are sold or offered for consumption, |
|  |  |  |
|  |  | (2) Inside equipment such as reach-in and under-counter refrigerators; and |
|  |  |  |
|  |  | (3) At a distance of 75 cm (30 inches) above the floor in areas used for handwashing, warewashing, and equipment and utensil storage, and in toilet rooms; and |
|  |  |  |
|  |  | (C) At least 540 lux (50 foot candles) at a surface where a food employee is working with food or working with utensils or equipment such as knives, slicers, grinders, or saws where employee safety is a factor. |