|  |
| --- |
| **4-204.116 Manual Warewashing Equipment, Heaters and Baskets.**  If hot water is used for sanitization in manual warewashing operations, the sanitizing compartment of the sink shall be: |
|  |
| (A) Designed with an integral heating device that is capable of maintaining water at a temperature not less than 77oC (171oF); Pf and |
| (B) Provided with a rack or basket to allow complete immersion of equipment and utensils into the hot water. Pf |