|  |
| --- |
| **5-202.12 Handwashing Sink, Installation.**  (A) A handwashing sink shall be equipped to provide water at a temperature of at least 38oC (100oF) through a mixing valve or combination faucet. Pf |
|  |
| (B) A steam mixing valve may not be used at a handwashing sink. |
|  |
| (C) A self-closing, slow-closing, or metering faucet shall provide a flow of water for at least 15 seconds without the need to reactivate the faucet. |
|  |
| (D) An automatic handwashing facility shall be installed in accordance with manufacturer’s instructions. |