|  |  |  |
| --- | --- | --- |
| ***Installation*** |  | **4-402.11 Fixed Equipment, Spacing or Sealing.**  (A) Equipment that is fixed because it is not easily movable shall be installed so that it is: |
|  |  |  |
|  |  | (1) Spaced to allow access for cleaning along the sides, behind, and above the equipment; |
|  |  |  |
|  |  | (2) Spaced from adjoining equipment, walls, and ceilings a distance of not more than 1 millimeter or one thirty-second inch; or |
|  |  |  |
|  |  | (3) Sealed to adjoining equipment or walls, if the equipment is exposed to spillage or seepage. |
|  |  |  |
|  |  | (B) Counter-mounted equipment that is not easily movable shall be installed to allow cleaning of the equipment and areas underneath and around the equipment by being: |
|  |  |  |
|  |  | (1) Sealed; or |
|  |  | (2) Elevated on legs as specified under ¶ 4-402.12(D). |