**6-501.16 Drying Mops.**

After use, mops shall be placed in a position that allows them to air-dry without soiling walls, equipment, or supplies.