|  |
| --- |
| **5-205.14 Water Reservoir of Fogging Devices, Cleaning.**  (A) A reservoir that is used to supply water to a device such as a produce fogger shall be: |
|  |
| (1) Maintained in accordance with manufacturer's specifications; P and |
|  |
| (2) Cleaned in accordance with manufacturer's specifications or according to the procedures specified under ¶ (B) of this section, whichever is more stringent. P |
|  |
| 1. Cleaning procedures shall include at least the following steps and shall be conducted at least once a week: |
|  |
| (1) Draining and complete disassembly of the water and aerosol contact parts; P |
|  |
| (2) Brush-cleaning the reservoir, aerosol tubing, and discharge nozzles with a suitable detergent solution; P |
|  |
| (3) Flushing the complete system with water to remove the detergent solution and particulate accumulation; P and |
|  |
| (4) Rinsing by immersing, spraying, or swabbing the reservoir, aerosol tubing, and discharge nozzles with at least 50 mg/L hypochlorite solution. P |