|  |
| --- |
| **5-203.15 Backflow Prevention Device, Carbonator.**  (A) If not provided with an air gap as specified under § 5-202.13, a dual check valve with an intermediate vent preceded by a screen of not less than 100 mesh to 25.4 mm (100 mesh to 1 inch) shall be installed upstream from a carbonating device and downstream from any copper in the water supply line. |
|  |
| (B) *A dual check valve attached to the carbonator need not be of the vented type if an air gap or vented backflow prevention device has been otherwise provided as specified under ¶ (A) of this section.* |