|  |
| --- |
| **5-203.14 Backflow Prevention Device, When Required.**  A plumbing system shall be installed to preclude backflow of a solid, liquid, or gas contaminant into the water supply system at each point of use at the food establishment, including on a hose bibb if a hose is attached or on a hose bibb if a hose is not attached and backflow prevention is required by law, by: |
|  |
| (A) Providing an air gap as specified under § 5‑202.13 P; or |
|  |
| (B) Installing an approved backflow prevention device as specified under § 5‑202.14. P |