|  |
| --- |
| **4-204.118 Warewashing Machines, Flow Pressure Device.**  (A) Warewashing machines that provide a fresh hot water sanitizing rinse shall be equipped with a pressure gauge or similar device such as a transducer that measures and displays the water pressure in the supply line immediately before entering the warewashing machine; and |
|  |
| (B) If the flow pressure measuring device is upstream of the fresh hot water sanitizing rinse control valve, the device shall be mounted in a 6.4 millimeter or one-fourth inch Iron Pipe Size (IPS) valve. |
|  |
| (C) *Paragraphs (A) and (B) of this section do not apply to a machine that uses only a pumped or recirculated sanitizing rinse.* |
|  |