|  |
| --- |
| **4-603.16 Rinsing Procedures.**  Washed utensils and equipment shall be rinsed so that abrasives are removed and cleaning chemicals are removed or diluted through the use of water or a detergent-sanitizer solution by using one of the following procedures: |
|  |
| (A) Use of a distinct, separate water rinse after washing and before sanitizing if using: |
|  |
| (1) A 3-compartment sink, |
|  |
| (2) Alternative manual warewashing equipment equivalent to a 3-compartment sink as specified in ¶ 4‑301.12(C), or |
|  |
| (3) A 3-step washing, rinsing, and sanitizing procedure in a warewashing system for cip equipment; |
|  |
| (B) Use of a detergent-sanitizer as specified under § 4‑501.115 if using: |
|  |
| (1) Alternative warewashing equipment as specified in ¶ 4‑301.12(C) that is approved for use with a detergent-sanitizer, or |
|  |
| (2) A warewashing system for cip equipment; |
|  |
| (C) Use of a nondistinct water rinse that is integrated in the hot water sanitization immersion step of a 2-compartment sink operation; |
|  |
| (D) If using a warewashing machine that does not recycle the sanitizing solution as specified under ¶ (E) of this section, or alternative manual warewashing equipment such as sprayers, use of a nondistinct water rinse that is: |
|  |
| (1) Integrated in the application of the sanitizing solution, and |
|  |
| (2) Wasted immediately after each application; or |
|  |
| (E) If using a warewashing machine that recycles the sanitizing solution for use in the next wash cycle, use of a nondistinct water rinse that is integrated in the application of the sanitizing solution. |