|  |  |
| --- | --- |
|  | **4-501.111 Manual Warewashing Equipment, Hot Water Sanitization Temperatures.**  If immersion in hot water is used for sanitizing in a manual operation, the temperature of the water shall be maintained at 77oC (171oF) or above. P |