|  |
| --- |
| **5-302.16 Hose, Construction and Identification.**  A hose used for conveying drinking water from a water tank shall be: |
|  |
| (A) Safe; P |
|  |
| (B) Durable, corrosion-resistant, and nonaborbent; |
|  |
| (C) Resistant to pitting, chipping, crazing, scratching, scoring, distortion, and decomposition; |
|  |
| (D) Finished with a smooth interior surface; and |
|  |
| (E) Clearly and durably identified as to its use if not permanently attached. |