|  |
| --- |
| **4-501.112 Mechanical Warewashing Equipment, Hot Water Sanitization Temperatures.**  (A) Except as specified in ¶ (B) of this section, in a mechanical operation, the temperature of the fresh hot water sanitizing rinse as it enters the manifold may not be more than 90oC (194oF), or less than: Pf |
|  |
| (1) For a stationary rack, single temperature machine, 74oC (165oF); Pf or |
|  |
| (2) For all other machines, 82oC (180oF). Pf |
|  |
| (B) *The maximum temperature specified under ¶ (A) of this section, does not apply to the high pressure and temperature systems with wand-type, hand-held, spraying devices used for the in-place cleaning and sanitizing of equipment such as meat saws.* |