**4-203.13 Pressure Measuring Devices, Mechanical Warewashing Equipment.**

Pressure measuring devices that display the pressures in the water supply line for the fresh hot water sanitizing rinse shall have increments of 7 kilopascals (1 pound per square inch) or smaller and shall be accurate to  ±14 kilopascals (~~~~ ±2 pounds per square inch) in the range indicated on the manufacturer’s data plate.