|  |  |  |
| --- | --- | --- |
| ***Operation and* *Maintenance*** |  | **5-304.11 System Flushing and Sanitization.**  A water tank, pump, and hoses shall be flushed and sanitized before being placed in service after construction, repair, modification, and periods of nonuse. P |