|  |
| --- |
| **5-302.15 Inlet and Outlet, Sloped to Drain.**  (A) A water tank and its inlet and outlet shall be sloped to drain. |
|  |
| (B) A water tank inlet shall be positioned so that it is protected from contaminants such as waste discharge, road dust, oil, or grease. |