|  |
| --- |
| **5-302.14 Tank Vent, Protected.**  If provided, a water tank vent shall terminate in a downward direction and shall be covered with: |
|  |
| (A) 16 mesh to 25.4 mm (16 mesh to 1 inch) screen or equivalent when the vent is in a protected area; or |
|  |
| (B) A protective filter when the vent is in an area that is not protected from windblown dirt and debris. |