|  |
| --- |
| **4-501.110 Mechanical Warewashing Equipment, Wash Solution Temperature.**  (A) The temperature of the wash solution in spray type warewashers that use hot water to sanitize may not be less than: |
|  |
| (1) For a stationary rack, single temperature machine, 74oC (165oF); Pf |
|  |
| (2) For a stationary rack, dual temperature machine, 66oC (150oF); Pf |
|  |
| (3) For a single tank, conveyor, dual temperature machine, 71oC (160oF); Pf or |
|  |
| (4) For a multitank, conveyor, multitemperature machine, 66oC (150oF). Pf |
|  |
| (B) The temperature of the wash solution in spray-type warewashers that use chemicals to sanitize may not be less than 49oC (120oF). Pf |