|  |
| --- |
| **4-203.12 Temperature Measuring Devices, Ambient Air and Water.**  (A) Ambient air and water temperature measuring devices that are scaled in Celsius or dually scaled in Celsius and Fahrenheit shall be designed to be easily readable and accurate to ±1.5oC in the intended range of use. Pf |
|  |
| (B) Ambient air and water temperature measuring devices that are scaled only in Fahrenheit shall be accurate to ±3oF in the intended range of use. Pf |