|  |
| --- |
| **6-201.16 Wall and Ceiling Coverings and Coatings.**  (A) Wall and ceiling covering materials shall be attached so that they are easily cleanable. |
|  |
| (B) *Except in areas used only for dry storage*, concrete, porous blocks, or bricks used for indoor wall construction shall be finished and sealed to provide a smooth, nonabsorbent, easily cleanable surface. |