|  |
| --- |
| **4-402.12 Fixed Equipment, Elevation or Sealing.**  (A) Except as specified in ¶¶ (B) and (C) of this section, floor-mounted equipment that is not easily movable shall be sealed to the floor or elevated on legs that provide at least a 15 centimeter (6 inch) clearance between the floor and the equipment. |
|  |
| (B) *If no part of the floor under the floor-mounted equipment is more than 15 centimeters (6 inches) from the point of cleaning access, the clearance space may be only 10 centimeters (4 inches)*. |
|  |
| (C) *This section does not apply to display shelving units, display refrigeration units, and display freezer units located in the consumer shopping areas of a retail food store, if the floor under the units is maintained clean*. |
|  |
| (D) Except as specified in ¶ (E) of this section, counter-mounted equipment that is not easily movable shall be elevated on legs that provide at least a 10 centimeter (4 inch) clearance between the table and the equipment. |
|  |
| (E) *The clearance space between the table and counter-mounted equipment may be*: |
|  |
| (1) *7.5 centimeters (3 inches) if the horizontal distance of the table top under the equipment is no more than 50 centimeters (20 inches) from the point of access for cleaning; or* |
|  |
| (2) *5 centimeters (2 inches) if the horizontal distance of the table top under the equipment is no more than 7.5 centimeters (3 inches) from the point of access for cleaning* |