|  |  |  |
| --- | --- | --- |
| ***Design and* *Construction*** |  | **5-302.11 Enclosed System, Sloped to Drain.**  A mobile water tank shall be: |
|  |  |  |
|  |  | (A) Enclosed from the filling inlet to the discharge outlet; and |
|  |  |  |
|  |  | (B) Sloped to an outlet that allows complete drainage of the tank. |