|  |
| --- |
| **6-301.12 Hand Drying Provision.**  Each handwashing sink or group of adjacent handwashing sinks shall be provided with: |
|  |
| (A) Individual, disposable towels; Pf |
|  |
| (B) A continuous towel system that supplies the user with a clean towel; Pf or |
|  |
| (C) A heated-air hand drying device; Pf or |
|  |
| (D) A hand drying device that employs an air-knife system that delivers high velocity, pressurized air at ambient temperatures. Pf |