|  |
| --- |
| **5-303.13 Mobile Food Establishment Tank Inlet.**  A mobile food establishment's water tank inlet shall be: |
|  |
| (A) 19.1 mm (three-fourths inch) in inner diameter or less; and |
|  |
| (B) Provided with a hose connection of a size or type that will prevent its use for any other service. |