|  |
| --- |
| **6-202.13 Insect Control Devices, Design and Installation.**  (A) Insect control devices that are used to electrocute or stun flying insects shall be designed to retain the insect within the device. |
|  |
|  |
| (B) Insect control devices shall be installed so that: |
|  |
| (1) The devices are not located over a food preparation area; and |
|  |
| (2) Dead insects and insect fragments are prevented from being impelled onto or falling on exposed food; clean equipment, utensils, and linens; and unwrapped single-service and single-use articles. |