|  |
| --- |
| **5-402.11 Backflow Prevention.**  (A) Except as specified in ¶¶ (B), (C), and (D) of this section, a direct connection may not exist between the sewage system and a drain originating from equipment in which food, portable equipment, or utensils are placed. P |
|  |
| (B) *Paragraph (A) of this section does not apply to floor drains that originate in refrigerated spaces that are constructed as an integral part of the building*. |
|  |
| (C) *If allowed by law, a warewashing machine may have a direct connection between its waste outlet and a floor drain when the machine is located within 1.5 m (5 feet) of a trapped floor drain and the machine outlet is connected to the inlet side of a properly vented floor drain trap.* |
|  |
| (D) *If allowed by law, a warewashing or culinary sink may have a direct connection*. |