|  |  |  |
| --- | --- | --- |
| ***Equipment*** |  | **4-501.11 Good Repair and Proper Adjustment.**  (A) Equipment shall be maintained in a state of repair and condition that meets the requirements specified under Parts 4‑1 and 4-2. |
|  |  |  |
|  |  | (B) Equipment components such as doors, seals, hinges, fasteners, and kick plates shall be kept intact, tight, and adjusted in accordance with manufacturer's specifications. |
|  |  |  |
|  |  | (C) Cutting or piercing parts of can openers shall be kept sharp to minimize the creation of metal fragments that can contaminate food when the container is opened. |