|  |
| --- |
| **4-202.12 CIP Equipment.**  (A) CIP equipment shall meet the characteristics specified under § 4‑202.11 and shall be designed and constructed so that: |
|  |
| (1) Cleaning and sanitizing solutions circulate throughout a fixed system and contact all interior food-contact surfaces, Pf and |
|  |
| (2) The system is self-draining or capable of being completely drained of cleaning and sanitizing solutions; and |
|  |
| (B) CIP equipment that is not designed to be disassembled for cleaning shall be designed with inspection access points to ensure that all interior food-contact surfaces throughout the fixed system are being effectively cleaned. |