|  |  |  |
| --- | --- | --- |
| ***Quantity and* *Availability*** |  | **5-103.11 Capacity.**  (A) The water source and system shall be of sufficient capacity to meet the peak water demands of the food establishment. Pf |
|  |  |  |
|  |  | (B) Hot water generation and distribution systems shall be sufficient to meet the peak hot water demands throughout the food establishment. Pf |