|  |  |  |
| --- | --- | --- |
| ***Mobile Holding Tank*** |  | **5-401.11 Capacity and Drainage.**  A sewage holding tank in a mobile food establishment shall be: |
|  |  |  |
|  |  | (A) Sized 15 percent larger in capacity than the water supply tank; and |
|  |  |  |
|  |  | (B) Sloped to a drain that is 25 mm (1 inch) in inner diameter or greater, equipped with a shut-off valve. |